Ener.co M&V Data Export
======================

Package Structure:
- summary.json        — Computed results (EER, savings, financials)
- project.json        — Raw project configuration and assumptions
- equipment_inventory.csv — Unit breakdown with factory specs
- financial_model.csv — Year-by-year CapEx deferral + R&M + energy savings
- ipmvp_assessment.json — Per-unit IPMVP compliance (regression, NMBE, FSU, DW)
- raw_data/           — Source CSV/JSON files

Methodology:
- IPMVP Option B (Retrofit Isolation, All Parameter Measurement)
- OAT-binned EER comparison (pre vs post treatment)
- Weather-normalized using multivariate OLS regression
- 15-minute averaged data buckets (aligned with utility metering)

Data Dictionary:
- eer_pre/eer_post: Mean EER before/after treatment (BTU/Wh)
- eer_pct_improvement: (post - pre) / pre × 100
- factory_eer: Manufacturer-rated EER at AHRI standard conditions
- delta_kw: Mean kW reduction at matched OAT conditions

Generated by Ener.co Refinery — https://ener.co
